<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="60.122" y2="0" width="0" layer="20"/>
<wire x1="60.122" y1="0" x2="60.122" y2="71.618" width="0" layer="20"/>
<wire x1="60.122" y1="71.618" x2="0" y2="71.618" width="0" layer="20"/>
<wire x1="0" y1="71.618" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="67.818" drill="2.8"/>
<hole x="56.388" y="67.818" drill="2.8"/>
<hole x="56.388" y="3.556" drill="2.8"/>
<hole x="3.556" y="3.556" drill="2.8"/>
</plain>
<libraries>
<library name="HyTechDevices">
<packages>
<package name="MINIFIT_5566-6">
<description>&lt;b&gt;Mini FIT connector 6 pol&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com</description>
</package>
<package name="MINIFIT_5566-4">
<description>&lt;b&gt;Mini FIT connector 4 pol&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com</description>
</package>
<package name="AXIAL-0.3">
</package>
<package name="ARDUINO_NANO">
</package>
<package name="CAP-PTH-SMALLEZ">
<description>This is the "EZ" version of the .1" spaced ceramic thru-hole cap.&lt;br&gt;
It has reduced top mask to make it harder to put the component on the wrong side of the board.</description>
</package>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="DG301-02P">
<description>DG301 2-Pin Terminal Block

&lt;br&gt;
&lt;br&gt;
These measurements should be close enough to place on a pcb</description>
</package>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle
&lt;br&gt;
&lt;a href="https://github.com/adafruit/Adafruit-Eagle-Library"&gt;Source: Adafruit&lt;/a&gt;</description>
</package>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="EXT_BOARD" library="HyTechDevices" package="MINIFIT_5566-6" value="MINIFIT_5566-6">
<attribute name="OC_NEWARK" value="22K8620"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="95566-61002"/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="MATRIX" library="HyTechDevices" package="MINIFIT_5566-4" value="MINIFIT_5566-4">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="HyTechDevices" package="AXIAL-0.3" value="10k"/>
<element name="R2" library="HyTechDevices" package="AXIAL-0.3" value="10k"/>
<element name="R3" library="HyTechDevices" package="AXIAL-0.3" value="10k"/>
<element name="U$1" library="HyTechDevices" package="ARDUINO_NANO" value="ARDUINO_NANO"/>
<element name="C1" library="HyTechDevices" package="CAP-PTH-SMALLEZ" value="100µF"/>
<element name="R4" library="HyTechDevices" package="AXIAL-0.3EZ" value="500"/>
<element name="R5" library="HyTechDevices" package="AXIAL-0.3EZ" value="500"/>
<element name="POWER_2" library="HyTechDevices" package="DG301-02P" value="TERMINAL_BLOCK_DG301-02P"/>
<element name="POWER_1" library="HyTechDevices" package="DCJACK_2MM_PTH" value=""/>
<element name="B5" library="HyTechDevices" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="B4" library="HyTechDevices" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="B3" library="HyTechDevices" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="B2" library="HyTechDevices" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="B1" library="HyTechDevices" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="B0" library="HyTechDevices" package="B3F-10XX" value="">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="R6" library="HyTechDevices" package="AXIAL-0.3EZ" value="10k"/>
<element name="R7" library="HyTechDevices" package="AXIAL-0.3EZ" value="10k"/>
<element name="R9" library="HyTechDevices" package="AXIAL-0.3EZ" value="10k"/>
<element name="R10" library="HyTechDevices" package="AXIAL-0.3EZ" value="10k"/>
<element name="R11" library="HyTechDevices" package="AXIAL-0.3EZ" value="10k"/>
<element name="R8" library="HyTechDevices" package="AXIAL-0.3EZ" value="10k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="MATRIX" pad="2"/>
<contactref element="EXT_BOARD" pad="2"/>
<contactref element="POWER_2" pad="2"/>
<contactref element="POWER_1" pad="GNDBREAK"/>
<contactref element="POWER_1" pad="GND"/>
<contactref element="U$1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R11" pad="P$2"/>
<contactref element="R10" pad="P$2"/>
<contactref element="R9" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R8" pad="P$2"/>
</signal>
<signal name="EXT_BOARD_LED_CTRL">
<contactref element="R5" pad="P$2"/>
<contactref element="EXT_BOARD" pad="3"/>
</signal>
<signal name="BTN_ENCODE1">
<contactref element="EXT_BOARD" pad="4"/>
<contactref element="U$1" pad="D4"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="BTN_ENCODE_2">
<contactref element="EXT_BOARD" pad="5"/>
<contactref element="U$1" pad="D3"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="MATRIX_LED_CTRL">
<contactref element="MATRIX" pad="3"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="BTN_ENCODE_3">
<contactref element="EXT_BOARD" pad="6"/>
<contactref element="U$1" pad="D2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="GND1"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="D6"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="EXT_BOARD_LED_CTRL_BEF_RES">
<contactref element="U$1" pad="D5"/>
<contactref element="R5" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="B5" pad="1"/>
<contactref element="R6" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="B4" pad="1"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="B3" pad="1"/>
<contactref element="R8" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="B2" pad="1"/>
<contactref element="R9" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="B1" pad="1"/>
<contactref element="R10" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="B0" pad="1"/>
<contactref element="R11" pad="P$1"/>
</signal>
<signal name="BTN0_IN">
<contactref element="B0" pad="2"/>
<contactref element="U$1" pad="A0"/>
</signal>
<signal name="BTN2_IN">
<contactref element="B2" pad="2"/>
<contactref element="U$1" pad="A2"/>
</signal>
<signal name="BTN3_IN">
<contactref element="B3" pad="2"/>
<contactref element="U$1" pad="A3"/>
</signal>
<signal name="BTN4_IN">
<contactref element="B4" pad="2"/>
<contactref element="U$1" pad="A4"/>
</signal>
<signal name="BTN5_IN">
<contactref element="B5" pad="2"/>
<contactref element="U$1" pad="A5"/>
</signal>
<signal name="BTN1_IN">
<contactref element="B1" pad="2"/>
<contactref element="U$1" pad="A1"/>
</signal>
<signal name="5V+">
<contactref element="POWER_1" pad="PWR"/>
<contactref element="B3" pad="3"/>
<contactref element="U$1" pad="VIN"/>
<contactref element="B1" pad="4"/>
<contactref element="POWER_2" pad="1"/>
<contactref element="B1" pad="3"/>
<contactref element="B2" pad="3"/>
<contactref element="EXT_BOARD" pad="1"/>
<contactref element="B5" pad="4"/>
<contactref element="B4" pad="4"/>
<contactref element="B0" pad="4"/>
<contactref element="MATRIX" pad="1"/>
<contactref element="B4" pad="3"/>
<contactref element="B0" pad="3"/>
<contactref element="B5" pad="3"/>
<contactref element="B2" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="B3" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
