<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="3.429" y1="0" x2="61.595" y2="0" width="0" layer="20"/>
<wire x1="65.024" y1="3.429" x2="65.024" y2="26.543" width="0" layer="20"/>
<wire x1="61.595" y1="29.972" x2="3.429" y2="29.972" width="0" layer="20"/>
<wire x1="0" y1="26.543" x2="0" y2="3.429" width="0" layer="20"/>
<wire x1="0" y1="3.429" x2="3.429" y2="0" width="0" layer="20" curve="90"/>
<wire x1="61.595" y1="0" x2="65.024" y2="3.429" width="0" layer="20" curve="90"/>
<wire x1="65.024" y1="26.543" x2="61.595" y2="29.972" width="0" layer="20" curve="90"/>
<wire x1="3.429" y1="29.972" x2="0" y2="26.543" width="0" layer="20" curve="90"/>
<hole x="3.556" y="26.543" drill="2.8956"/>
<hole x="3.556" y="3.429" drill="2.8956"/>
<hole x="61.468" y="3.429" drill="2.8956"/>
<hole x="61.468" y="26.543" drill="2.8956"/>
<text>CAN shield rev2
Nathan Cheek &amp; Ryan Gallaway</text>
<text>Nothing to see here...</text>
<text>CANL</text>
<text>CANH</text>
<text>GND</text>
<text>CAN</text>
</plain>
<libraries>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="HyTechDevices">
<packages>
<package name="MINIFIT_5566-4">
<description>&lt;b&gt;Mini-Fit Junior connector 4 pole&lt;/b&gt;&lt;p&gt;
Source: http://www.molex.com</description>
</package>
<package name="SOIC-08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="TSSOP-20">
<description>&lt;b&gt;24-Lead Thin Shrink Small Outline Package TSSOP&lt;/b&gt; (RU-24)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/39677768AD7714_c.pdf</description>
</package>
<package name="0805">
</package>
<package name="LED-805">
<description>LED 805 Surface Mount
&lt;br&gt;
&lt;a href="https://github.com/DangerousPrototypes/Eagle_Part_Library"&gt;Source: Dangerous Prototypes Eagle Library&lt;/a&gt;</description>
</package>
<package name="TO-220-H">
<description>&lt;b&gt;TO 220 horizontal&lt;/b&gt;
&lt;br&gt;
Source: transistor-fet.lbr</description>
</package>
<package name="1X20">
</package>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="DO-41">
<description>DO-41
&lt;br&gt;
&lt;br&gt;
DIODE
&lt;br&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="F09HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CRYSTAL" library="SparkFun-FreqCtrl" package="HC49UP" value="16MHz"/>
<element name="EXTERNAL_1" library="HyTechDevices" package="MINIFIT_5566-4" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="MCP2551" library="HyTechDevices" package="SOIC-08" value="MCP2551"/>
<element name="MCP2515" library="HyTechDevices" package="TSSOP-20" value="MCP2515TSSOP"/>
<element name="R1" library="HyTechDevices" package="0805" value="100"/>
<element name="R2" library="HyTechDevices" package="0805" value="100"/>
<element name="R3" library="HyTechDevices" package="0805" value="4.7k"/>
<element name="C2" library="HyTechDevices" package="0805" value=".1uF"/>
<element name="C1" library="HyTechDevices" package="0805" value=".33uF"/>
<element name="C3" library="HyTechDevices" package="0805" value="560pF"/>
<element name="C4" library="HyTechDevices" package="0805" value="560pF"/>
<element name="C6" library="HyTechDevices" package="0805" value="22pF"/>
<element name="C7" library="HyTechDevices" package="0805" value="22pF"/>
<element name="LED1" library="HyTechDevices" package="LED-805" value=""/>
<element name="R4" library="HyTechDevices" package="0805" value="150"/>
<element name="LED3" library="HyTechDevices" package="LED-805" value=""/>
<element name="R6" library="HyTechDevices" package="0805" value="150"/>
<element name="IC1" library="HyTechDevices" package="TO-220-H" value=""/>
<element name="LED2" library="HyTechDevices" package="LED-805" value=""/>
<element name="R5" library="HyTechDevices" package="0805" value="150"/>
<element name="PI_EVEN" library="HyTechDevices" package="1X20" value=""/>
<element name="PI_ODD" library="HyTechDevices" package="1X20" value=""/>
<element name="BUTTON" library="HyTechDevices" package="B3F-10XX" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="OC_NEWARK" value="36M3542"/>
</element>
<element name="JP1" library="HyTechDevices" package="1X02" value="M02"/>
<element name="DB9" library="HyTechDevices" package="F09HP" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="CANL_JMP" library="HyTechDevices" package="1X03" value=""/>
<element name="CANH_JMP" library="HyTechDevices" package="1X03" value=""/>
<element name="GND_JMP" library="HyTechDevices" package="1X03" value=""/>
<element name="D1" library="HyTechDevices" package="DO-41" value="DIODEDO-41"/>
<element name="R7" library="HyTechDevices" package="0805" value="120"/>
</elements>
<signals>
<signal name="GND">
<contactref element="MCP2551" pad="2"/>
<contactref element="MCP2515" pad="10"/>
<contactref element="EXTERNAL_1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="PI_EVEN" pad="3"/>
<contactref element="BUTTON" pad="1"/>
<contactref element="GND_JMP" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="MCP2551" pad="1"/>
<contactref element="MCP2515" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="MCP2551" pad="4"/>
<contactref element="MCP2515" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="CRYSTAL" pad="2"/>
<contactref element="MCP2515" pad="9"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="MCP2551" pad="8"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="CRYSTAL" pad="1"/>
<contactref element="MCP2515" pad="8"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="R2" pad="1"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="CS">
<contactref element="MCP2515" pad="18"/>
<contactref element="PI_EVEN" pad="12"/>
</signal>
<signal name="MISO">
<contactref element="MCP2515" pad="17"/>
<contactref element="PI_ODD" pad="11"/>
</signal>
<signal name="MOSI">
<contactref element="MCP2515" pad="16"/>
<contactref element="PI_ODD" pad="10"/>
</signal>
<signal name="SCK">
<contactref element="MCP2515" pad="14"/>
<contactref element="PI_ODD" pad="12"/>
</signal>
<signal name="INT">
<contactref element="MCP2515" pad="13"/>
<contactref element="PI_EVEN" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="LED3" pad="C"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="MCP2551" pad="3"/>
<contactref element="MCP2515" pad="19"/>
<contactref element="MCP2515" pad="20"/>
<contactref element="C2" pad="1"/>
<contactref element="LED3" pad="A"/>
<contactref element="IC1" pad="3"/>
<contactref element="PI_EVEN" pad="1"/>
</signal>
<signal name="LED2">
<contactref element="LED2" pad="A"/>
<contactref element="PI_ODD" pad="18"/>
</signal>
<signal name="LED1">
<contactref element="LED1" pad="A"/>
<contactref element="PI_ODD" pad="19"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="C"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="BUT">
<contactref element="PI_EVEN" pad="18"/>
<contactref element="BUTTON" pad="4"/>
</signal>
<signal name="CANL">
<contactref element="JP1" pad="1"/>
<contactref element="CANL_JMP" pad="2"/>
<contactref element="MCP2551" pad="6"/>
<contactref element="EXTERNAL_1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="CANH">
<contactref element="JP1" pad="2"/>
<contactref element="CANH_JMP" pad="2"/>
<contactref element="MCP2551" pad="7"/>
<contactref element="EXTERNAL_1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="DB9" pad="9"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="P3">
<contactref element="DB9" pad="3"/>
<contactref element="CANH_JMP" pad="1"/>
<contactref element="GND_JMP" pad="3"/>
</signal>
<signal name="P5">
<contactref element="DB9" pad="5"/>
<contactref element="CANL_JMP" pad="1"/>
</signal>
<signal name="P2">
<contactref element="DB9" pad="2"/>
<contactref element="CANL_JMP" pad="3"/>
<contactref element="GND_JMP" pad="1"/>
</signal>
<signal name="P7">
<contactref element="DB9" pad="7"/>
<contactref element="CANH_JMP" pad="3"/>
</signal>
<signal name="+12V">
<contactref element="D1" pad="C"/>
<contactref element="EXTERNAL_1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
