<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="97.822" y1="0" x2="1.822" y2="0" width="0" layer="20"/>
<wire x1="-0.178" y1="2" x2="-0.178" y2="98" width="0" layer="20"/>
<hole x="95.822" y="4" drill="3.3"/>
<hole x="3.822" y="4" drill="3.3"/>
<hole x="3.822" y="96" drill="3.3"/>
<hole x="95.822" y="96" drill="3.3"/>
<wire x1="1.822" y1="100" x2="97.822" y2="100" width="0" layer="20"/>
<wire x1="99.822" y1="98" x2="99.822" y2="2" width="0" layer="20"/>
<wire x1="99.822" y1="98" x2="97.822" y2="100" width="0" layer="20" curve="90"/>
<wire x1="97.822" y1="0" x2="99.822" y2="2" width="0" layer="20" curve="90"/>
<wire x1="-0.178" y1="2" x2="1.822" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.822" y1="100" x2="-0.178" y2="98" width="0" layer="20" curve="90"/>
<text>PROG</text>
<text>RST</text>
<text>SET1</text>
<text>SET2</text>
<text>Nathan Cheek
nathancheek.com
Matrix Segment rev1
2018</text>
</plain>
<libraries>
<library name="HyTechDevices">
<packages>
<package name="0805">
</package>
<package name="LED_RGB_8MM">
</package>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;
&lt;br&gt;
&lt;a href="https://github.com/adafruit/Adafruit-Eagle-Library"&gt;Source: Adafruit&lt;/a&gt;</description>
</package>
<package name="TEENSY_3.2_SIMPLE_SMD">
</package>
<package name="SOT-23-5">
<description>&lt;a href="https://github.com/open-ephys/eagle-libraries"&gt;Source&lt;/a&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SOIC-08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="ESP8266_ESP-07_SMD">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;
&lt;br&gt;
&lt;a href="https://github.com/sparkfun/SparkFun-Eagle-Libraries"&gt;Source: Sparkfun Eagle Library</description>
</package>
<package name="TACTILE_SWITCH_SMD_6.2MM_TALL">
<description>Source: Sparkfun Library

&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.apem.com/files/apem/brochures/ADTS6-ADTSM-KTSC6.pdf"&gt;Datasheet&lt;/a&gt; (ADTSM63NVTR)&lt;/p&gt;</description>
</package>
<package name="CAP-PTH-5MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C10" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C11" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C12" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C13" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C14" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C15" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C16" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C17" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C18" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C19" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C2" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C20" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C21" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C22" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C23" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C24" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C25" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C3" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C4" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C5" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C6" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C7" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C8" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="C9" library="HyTechDevices" package="0805" value=".1µF"/>
<element name="U$1" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$10" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$11" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$12" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$13" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$14" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$15" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$16" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$17" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$18" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$19" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$2" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$20" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$21" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$22" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$23" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$24" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$25" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$3" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$4" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$5" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$6" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$7" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$8" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="U$9" library="HyTechDevices" package="LED_RGB_8MM" value="APA106_8MM"/>
<element name="CN1" library="HyTechDevices" package="DCJACK_2MM_SMT" value=""/>
<element name="U$26" library="HyTechDevices" package="TEENSY_3.2_SIMPLE_SMD" value="TEENSY_3.2_SIMPLESMD"/>
<element name="U$27" library="HyTechDevices" package="SOT-23-5" value="SN74LV1T34"/>
<element name="JP1" library="HyTechDevices" package="1X06" value=""/>
<element name="JP2" library="HyTechDevices" package="1X06" value=""/>
<element name="JP3" library="HyTechDevices" package="1X06" value=""/>
<element name="JP4" library="HyTechDevices" package="1X06" value=""/>
<element name="U$28" library="HyTechDevices" package="SOIC-08" value="MCP2551"/>
<element name="R1" library="HyTechDevices" package="0805" value="120"/>
<element name="U$29" library="HyTechDevices" package="ESP8266_ESP-07_SMD" value="ESP8266_ESP-07_SMD"/>
<element name="U$30" library="HyTechDevices" package="SOT223" value="TLV1117LV33"/>
<element name="R2" library="HyTechDevices" package="0805" value="10k"/>
<element name="R3" library="HyTechDevices" package="0805" value="10k"/>
<element name="PRGM" library="HyTechDevices" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value=""/>
<element name="R4" library="HyTechDevices" package="0805" value="10k"/>
<element name="RST" library="HyTechDevices" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value=""/>
<element name="R5" library="HyTechDevices" package="0805" value="10k"/>
<element name="C26" library="HyTechDevices" package="0805" value="1µF"/>
<element name="C27" library="HyTechDevices" package="0805" value="1µF"/>
<element name="SET1" library="HyTechDevices" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value=""/>
<element name="SET2" library="HyTechDevices" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value=""/>
<element name="R6" library="HyTechDevices" package="0805" value="330"/>
<element name="C28" library="HyTechDevices" package="CAP-PTH-5MM" value="1000µF"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U$1" pad="P$4"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="P$4"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="P$4"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="U$5" pad="P$1"/>
<contactref element="U$4" pad="P$4"/>
</signal>
<signal name="N$5">
<contactref element="U$6" pad="P$4"/>
<contactref element="U$7" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="U$7" pad="P$4"/>
<contactref element="U$8" pad="P$1"/>
</signal>
<signal name="N$7">
<contactref element="U$8" pad="P$4"/>
<contactref element="U$9" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="U$10" pad="P$1"/>
<contactref element="U$9" pad="P$4"/>
</signal>
<signal name="N$9">
<contactref element="U$11" pad="P$4"/>
<contactref element="U$12" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="U$12" pad="P$4"/>
<contactref element="U$13" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="U$13" pad="P$4"/>
<contactref element="U$14" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="U$15" pad="P$1"/>
<contactref element="U$14" pad="P$4"/>
</signal>
<signal name="N$13">
<contactref element="U$16" pad="P$4"/>
<contactref element="U$17" pad="P$1"/>
</signal>
<signal name="N$14">
<contactref element="U$17" pad="P$4"/>
<contactref element="U$18" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="U$18" pad="P$4"/>
<contactref element="U$19" pad="P$1"/>
</signal>
<signal name="N$16">
<contactref element="U$20" pad="P$1"/>
<contactref element="U$19" pad="P$4"/>
</signal>
<signal name="N$17">
<contactref element="U$21" pad="P$4"/>
<contactref element="U$22" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="U$22" pad="P$4"/>
<contactref element="U$23" pad="P$1"/>
</signal>
<signal name="N$19">
<contactref element="U$23" pad="P$4"/>
<contactref element="U$24" pad="P$1"/>
</signal>
<signal name="N$20">
<contactref element="U$25" pad="P$1"/>
<contactref element="U$24" pad="P$4"/>
</signal>
<signal name="N$21">
<contactref element="U$5" pad="P$4"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="U$10" pad="P$4"/>
<contactref element="U$11" pad="P$1"/>
</signal>
<signal name="N$23">
<contactref element="U$15" pad="P$4"/>
<contactref element="U$16" pad="P$1"/>
</signal>
<signal name="N$24">
<contactref element="U$20" pad="P$4"/>
<contactref element="U$21" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$5" pad="P$3"/>
<contactref element="U$10" pad="P$3"/>
<contactref element="U$9" pad="P$3"/>
<contactref element="U$8" pad="P$3"/>
<contactref element="U$7" pad="P$3"/>
<contactref element="U$6" pad="P$3"/>
<contactref element="U$11" pad="P$3"/>
<contactref element="U$12" pad="P$3"/>
<contactref element="U$13" pad="P$3"/>
<contactref element="U$14" pad="P$3"/>
<contactref element="U$15" pad="P$3"/>
<contactref element="U$20" pad="P$3"/>
<contactref element="U$25" pad="P$3"/>
<contactref element="U$24" pad="P$3"/>
<contactref element="U$19" pad="P$3"/>
<contactref element="U$18" pad="P$3"/>
<contactref element="U$23" pad="P$3"/>
<contactref element="U$21" pad="P$3"/>
<contactref element="U$22" pad="P$3"/>
<contactref element="U$17" pad="P$3"/>
<contactref element="U$16" pad="P$3"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="CN1" pad="GND"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP2" pad="6"/>
<contactref element="JP3" pad="6"/>
<contactref element="JP4" pad="6"/>
<contactref element="U$26" pad="GND"/>
<contactref element="U$28" pad="8"/>
<contactref element="U$28" pad="2"/>
<contactref element="U$28" pad="5"/>
<contactref element="U$27" pad="3"/>
<contactref element="U$30" pad="1"/>
<contactref element="U$29" pad="P$9"/>
<contactref element="R2" pad="2"/>
<contactref element="PRGM" pad="B2"/>
<contactref element="RST" pad="B2"/>
<contactref element="CN1" pad="GNDBREAK"/>
<contactref element="C26" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="SET1" pad="B2"/>
<contactref element="SET2" pad="B2"/>
<contactref element="C28" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="C2" pad="1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="C3" pad="1"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="C4" pad="1"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="C5" pad="1"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="C10" pad="1"/>
<contactref element="U$10" pad="P$2"/>
<contactref element="C9" pad="1"/>
<contactref element="U$9" pad="P$2"/>
<contactref element="C8" pad="1"/>
<contactref element="U$8" pad="P$2"/>
<contactref element="C7" pad="1"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="C6" pad="1"/>
<contactref element="U$6" pad="P$2"/>
<contactref element="C11" pad="1"/>
<contactref element="U$11" pad="P$2"/>
<contactref element="C12" pad="1"/>
<contactref element="U$12" pad="P$2"/>
<contactref element="C13" pad="1"/>
<contactref element="U$13" pad="P$2"/>
<contactref element="C14" pad="1"/>
<contactref element="U$14" pad="P$2"/>
<contactref element="C15" pad="1"/>
<contactref element="U$15" pad="P$2"/>
<contactref element="C16" pad="1"/>
<contactref element="U$16" pad="P$2"/>
<contactref element="C17" pad="1"/>
<contactref element="U$17" pad="P$2"/>
<contactref element="C18" pad="1"/>
<contactref element="U$18" pad="P$2"/>
<contactref element="C19" pad="1"/>
<contactref element="U$19" pad="P$2"/>
<contactref element="C20" pad="1"/>
<contactref element="U$20" pad="P$2"/>
<contactref element="C21" pad="1"/>
<contactref element="U$21" pad="P$2"/>
<contactref element="C22" pad="1"/>
<contactref element="U$22" pad="P$2"/>
<contactref element="C23" pad="1"/>
<contactref element="U$23" pad="P$2"/>
<contactref element="C24" pad="1"/>
<contactref element="U$24" pad="P$2"/>
<contactref element="C25" pad="1"/>
<contactref element="U$25" pad="P$2"/>
<contactref element="CN1" pad="PWR1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="U$26" pad="VIN"/>
<contactref element="U$28" pad="3"/>
<contactref element="U$27" pad="5"/>
<contactref element="U$30" pad="3"/>
<contactref element="C26" pad="1"/>
<contactref element="C28" pad="1"/>
</signal>
<signal name="DIN">
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP4" pad="2"/>
<contactref element="U$27" pad="4"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="DOUT">
<contactref element="U$25" pad="P$4"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="CANL">
<contactref element="JP1" pad="4"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP4" pad="4"/>
<contactref element="U$28" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="CANH">
<contactref element="JP1" pad="5"/>
<contactref element="JP2" pad="5"/>
<contactref element="JP3" pad="5"/>
<contactref element="JP4" pad="5"/>
<contactref element="U$28" pad="7"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="U$26" pad="D3(CANTX)"/>
<contactref element="U$28" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="U$26" pad="D4(CANRX)"/>
<contactref element="U$28" pad="4"/>
</signal>
<signal name="N$27">
<contactref element="U$27" pad="2"/>
<contactref element="U$26" pad="D12"/>
</signal>
<signal name="+3V3">
<contactref element="U$30" pad="4"/>
<contactref element="U$30" pad="2"/>
<contactref element="U$29" pad="P$8"/>
<contactref element="U$29" pad="P$3"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="ESP_TX">
<contactref element="U$29" pad="P$16"/>
<contactref element="U$26" pad="D9(RX2)"/>
</signal>
<signal name="ESP_RX">
<contactref element="U$29" pad="P$15"/>
<contactref element="U$26" pad="D10(TX2)"/>
</signal>
<signal name="N$28">
<contactref element="R2" pad="1"/>
<contactref element="U$29" pad="P$10"/>
</signal>
<signal name="N$29">
<contactref element="U$29" pad="P$11"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="U$29" pad="P$12"/>
<contactref element="PRGM" pad="A2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="U$29" pad="P$1"/>
<contactref element="RST" pad="A2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="SET1" pad="A2"/>
<contactref element="U$26" pad="A6"/>
</signal>
<signal name="N$33">
<contactref element="SET2" pad="A2"/>
<contactref element="U$26" pad="A5"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="P$1"/>
<contactref element="R6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
